# Transfer

* You are on a call
* Choose ***Consult*** from the on screen menu by pressing OK
* Dial another number and either
  + Wait for answer announce then hang up
  + If the call is not wanted choose ***Drop and return***
  + Or Hangup to transfer

# Transfer – Blind

* You are on a call
* Choose ***Transfer*** from the on screen menu and press OK
* Dial another number and press OK
* The call is transferred immediately

# Call Pickup

* Another phone in you group is ringing
* The screen will prompt for a call pick up, Press OK

# Call Park

* You are on a call
* Choose ***Consult*** from the on screen menu by pressing OK
* Dial \*56 and listen to the announcement (or \*\* in some cases)
* Your call is now parked

# Park Retrieve

* Your phone is free
* Dial #56 (or \*# in some cases) and dial the park location then ***#***
* Your call is now retrieved

The following feature need to be pre-programed.

# Broadcast

* \*87 + X where X = paging zone

# 1-way intercom

* \*80 + XX where XX=destination shortcut

# 2-way intercom

* \*88 + XX where XX=destination shortcut

# Voicemail Phone Mode

* The message key will light if you have voicemail
* Press the message key
* First time users will be prompted to set a PIN, name and greeting  
  *Please note your name is not your greeting!*
* You may be prompted for a PIN (optional)
* Follow the instruction given to play/delete messages

Voicemail Web-UC Mode

* The message key will light if you have voicemail
* Press the message key
* You can play your greeting
* Your name and Greeting are set via the web service

Key Programming

* Hold the key down for 5 seconds
* Choose OK to program
* Change Unallocated to the feature you require (usually Selected Dialling)

First